<?xml version="1.0" ?>
<robot name="iisy">
  <link name="world"/>
  <link name="base_link"/>
  <link name="table">
    <collision>
      <geometry>
        <mesh filename="file://$(find iisy_config)/stl/table.stl"/>
      </geometry>
    </collision>
    <visual>
      <geometry>
        <mesh filename="file://$(find iisy_config)/stl/table.stl"/>
      </geometry>
    </visual>
  </link>
  <link name="base_bottom">
    <collision>
      <geometry>
        <mesh filename="file://$(find iisy_config)/stl/base_bottom_coll.stl"/>
      </geometry>
    </collision>
    <visual>
      <geometry>
        <mesh filename="file://$(find iisy_config)/stl/base_bottom_low.stl"/>
      </geometry>
    </visual>
    <inertial>
      <origin rpy="0 0 0" xyz="-0.043517 0.000000 0.054914"/>
      <mass value="0.1"/>
      <inertia ixx="1.277905" ixy="0.0" ixz="0.138279" iyy="3.070705" iyz="0.0" izz="3.284356"/>
    </inertial>
  </link>
  <link name="base_top">
    <collision>
      <origin xyz="0 -0.005 0.08"/>
      <geometry>
        <box size="0.14 0.15 0.16"/>
      </geometry>
    </collision>
    <visual>
      <geometry>
        <mesh filename="file://$(find iisy_config)/stl/base_top_low.stl"/>
      </geometry>
    </visual>
    <inertial>
      <origin rpy="0 0 0" xyz="0 -0.005 0.08"/>
      <mass value="0.1"/>
      <inertia ixx="0.32666666666667" ixy="0.0" ixz="0.0" iyy="0.32666666666667" iyz="0.0" izz="0.25"/>
    </inertial>
  </link>
  <link name="link1_full">
    <collision>
      <geometry>
        <mesh filename="file://$(find iisy_config)/stl/link_1_full_coll.stl"/>
      </geometry>
    </collision>
    <visual>
      <geometry>
        <mesh filename="file://$(find iisy_config)/stl/link_1_full_low.stl"/>
      </geometry>
    </visual>
    <inertial>
      <origin rpy="0 0 0" xyz="0 -0.050000 0.150000"/>
      <mass value="0.1"/>
      <inertia ixx="8.266347" ixy="0.0" ixz="0.0" iyy="8.647519" iyz="0.0" izz="8.647519"/>
    </inertial>
  </link>
  <link name="link2_bottom">
    <collision>
      <origin xyz="0 0.07 0.025"/>
      <geometry>
        <box size="0.14 0.14 0.19"/>
      </geometry>
    </collision>
    <visual>
      <geometry>
        <mesh filename="file://$(find iisy_config)/stl/link_2_bottom_low.stl"/>
      </geometry>
    </visual>
    <inertial>
      <origin rpy="0 0 0" xyz="0 0.07 0.025"/>
      <mass value="0.1"/>
      <inertia ixx="0.5" ixy="0.0" ixz="0.0" iyy="0.5" iyz="0.0" izz="0.25"/>
    </inertial>
  </link>
  <link name="link2_top">
    <collision>
      <geometry>
        <mesh filename="file://$(find iisy_config)/stl/link_2_top_coll.stl"/>
      </geometry>
    </collision>
    <visual>
      <geometry>
        <mesh filename="file://$(find iisy_config)/stl/link_2_top_low.stl"/>
      </geometry>
    </visual>
    <inertial>
      <origin rpy="0 0 0" xyz="0 0.037363 0.086674"/>
      <mass value="0.1"/>
      <inertia ixx="1.431738" ixy="0.0" ixz="0.0" iyy="1.131426" iyz="-0.342192" izz="0.807202"/>
    </inertial>
  </link>
  <link name="link3_bottom">
    <collision>
      <geometry>
        <mesh filename="file://$(find iisy_config)/stl/link_3_bottom_coll.stl"/>
      </geometry>
    </collision>
    <visual>
      <geometry>
        <mesh filename="file://$(find iisy_config)/stl/link_3_bottom_low.stl"/>
      </geometry>
    </visual>
    <inertial>
      <origin rpy="0 0 0" xyz="0 -0.055000 0.021413"/>
      <mass value="0.1"/>
      <inertia ixx="0.362124" ixy="0.0" ixz="0.0" iyy="0.343531" iyz="0.0" izz="0.283368"/>
    </inertial>
  </link>
  <link name="link3_top">
    <collision>
      <geometry>
        <mesh filename="file://$(find iisy_config)/stl/link_3_top_coll.stl"/>
      </geometry>
    </collision>
    <visual>
      <geometry>
        <mesh filename="file://$(find iisy_config)/stl/link_3_top_low.stl"/>
      </geometry>
    </visual>
    <inertial>
      <origin rpy="0 0 0" xyz="0 -0.015462 0.040000"/>
      <mass value="0.1"/>
      <inertia ixx="0.228470" ixy="0.0" ixz="0.0" iyy="0.137641" iyz="0.0" izz="0.252003"/>
    </inertial>
  </link>
  <joint name="world_base_link_fixed" type="fixed">
    <origin rpy="0 0 0" xyz="0 0 0"/>
    <parent link="world"/>
    <child link="base_link"/>
  </joint>
  <joint name="base_base_link_fixed" type="fixed">
    <origin rpy="0 0 0" xyz="0 0 0"/>
    <parent link="base_link"/>
    <child link="table"/>
  </joint>
  <joint name="table_link_fixed" type="fixed">
    <origin rpy="0 0 0" xyz="0 0 1"/>
    <parent link="table"/>
    <child link="base_bottom"/>
  </joint>
  <joint name="base_rot" type="continuous">
    <origin rpy="0 0 0" xyz="0 0 0.1205"/>
    <parent link="base_bottom"/>
    <child link="base_top"/>
    <axis xyz="0 0 1"/>
    <limit effort="30" velocity="1.7453292519943"/>
    <dynamics damping="10.0" friction="0.1"/>
  </joint>
  <joint name="base_link1_joint" type="revolute">
    <origin rpy="0 0 0" xyz="0 -0.080499 0.092997"/>
    <parent link="base_top"/>
    <child link="link1_full"/>
    <axis xyz="0 1 0"/>
    <limit effort="30" lower="-2.2689280275926" upper="2.4434609527921" velocity="1.7453292519943"/>
    <dynamics damping="10.0" friction="0.1"/>
  </joint>
  <joint name="link1_link2_joint" type="revolute">
    <origin rpy="0 0 0" xyz="0 0 0.3"/>
    <parent link="link1_full"/>
    <child link="link2_bottom"/>
    <axis xyz="0 1 0"/>
    <limit effort="30" lower="-2.6179938779915" upper="2.6179938779915" velocity="1.7453292519943"/>
    <dynamics damping="10.0" friction="0.1"/>
  </joint>
  <joint name="link2_rot" type="continuous">
    <origin rpy="0 0 0" xyz="0 0.080501 0.120502"/>
    <parent link="link2_bottom"/>
    <child link="link2_top"/>
    <axis xyz="0 0 1"/>
    <limit effort="30" velocity="1.7453292519943"/>
    <dynamics damping="10.0" friction="0.1"/>
  </joint>
  <joint name="link2_link3_joint" type="continuous">
    <origin rpy="0 0 0" xyz="0 0.0565 0.178003"/>
    <parent link="link2_top"/>
    <child link="link3_bottom"/>
    <axis xyz="0 1 0"/>
    <limit effort="30" velocity="1.7453292519943"/>
    <dynamics damping="10.0" friction="0.1"/>
  </joint>
  <joint name="link3_rot" type="continuous">
    <origin rpy="0 0 0" xyz="0 -0.055001 0.085501"/>
    <parent link="link3_bottom"/>
    <child link="link3_top"/>
    <axis xyz="0 0 1"/>
    <limit effort="30" velocity="1.7453292519943"/>
    <dynamics damping="10.0" friction="0.1"/>
  </joint>
  <transmission name="trans_base_rot">
    <type>transmission_interface/SimpleTransmission</type>
    <joint name="base_rot">
      <hardwareInterface>hardware_interface/EffortJointInterface</hardwareInterface>
    </joint>
    <actuator name="base_rot_motor">
      <hardwareInterface>hardware_interface/EffortJointInterface</hardwareInterface>
      <mechanicalReduction>1</mechanicalReduction>
    </actuator>
  </transmission>
  <transmission name="trans_base_link1_joint">
    <type>transmission_interface/SimpleTransmission</type>
    <joint name="base_link1_joint">
      <hardwareInterface>hardware_interface/EffortJointInterface</hardwareInterface>
    </joint>
    <actuator name="base_link1_joint_motor">
      <hardwareInterface>hardware_interface/EffortJointInterface</hardwareInterface>
      <mechanicalReduction>1</mechanicalReduction>
    </actuator>
  </transmission>
  <transmission name="trans_link1_link2_joint">
    <type>transmission_interface/SimpleTransmission</type>
    <joint name="link1_link2_joint">
      <hardwareInterface>hardware_interface/EffortJointInterface</hardwareInterface>
    </joint>
    <actuator name="link1_link2_joint_motor">
      <hardwareInterface>hardware_interface/EffortJointInterface</hardwareInterface>
      <mechanicalReduction>1</mechanicalReduction>
    </actuator>
  </transmission>
  <transmission name="trans_link2_rot">
    <type>transmission_interface/SimpleTransmission</type>
    <joint name="link2_rot">
      <hardwareInterface>hardware_interface/EffortJointInterface</hardwareInterface>
    </joint>
    <actuator name="link2_rot_motor">
      <hardwareInterface>hardware_interface/EffortJointInterface</hardwareInterface>
      <mechanicalReduction>1</mechanicalReduction>
    </actuator>
  </transmission>
  <transmission name="trans_link2_link3_joint">
    <type>transmission_interface/SimpleTransmission</type>
    <joint name="link2_link3_joint">
      <hardwareInterface>hardware_interface/EffortJointInterface</hardwareInterface>
    </joint>
    <actuator name="link2_link3_joint_motor">
      <hardwareInterface>hardware_interface/EffortJointInterface</hardwareInterface>
      <mechanicalReduction>1</mechanicalReduction>
    </actuator>
  </transmission>
  <transmission name="trans_link3_rot">
    <type>transmission_interface/SimpleTransmission</type>
    <joint name="link3_rot">
      <hardwareInterface>hardware_interface/EffortJointInterface</hardwareInterface>
    </joint>
    <actuator name="link3_rot_motor">
      <hardwareInterface>hardware_interface/EffortJointInterface</hardwareInterface>
      <mechanicalReduction>1</mechanicalReduction>
    </actuator>
  </transmission>
  <gazebo reference="base_bottom">
    <mu1>0.2</mu1>
    <mu2>0.2</mu2>
    <material>Gazebo/Orange</material>
  </gazebo>
  <gazebo reference="base_top">
    <mu1>0.2</mu1>
    <mu2>0.2</mu2>
    <material>Gazebo/Orange</material>
  </gazebo>
  <gazebo reference="link1_full">
    <mu1>0.2</mu1>
    <mu2>0.2</mu2>
    <material>Gazebo/Orange</material>
  </gazebo>
  <gazebo reference="link2_bottom">
    <mu1>0.2</mu1>
    <mu2>0.2</mu2>
    <material>Gazebo/Orange</material>
  </gazebo>
  <gazebo reference="link2_top">
    <mu1>0.2</mu1>
    <mu2>0.2</mu2>
    <material>Gazebo/Orange</material>
  </gazebo>
  <gazebo reference="link3_bottom">
    <mu1>0.2</mu1>
    <mu2>0.2</mu2>
    <material>Gazebo/Orange</material>
  </gazebo>
  <gazebo reference="link3_top">
    <mu1>0.2</mu1>
    <mu2>0.2</mu2>
    <material>Gazebo/Grey</material>
  </gazebo>
</robot>
